# SmartCard AFNOR

     -------------+-------------
    |   8         |         4   |
    |             |             |
    +-------\     |     /-------+
    |   7    +----+----+    3   |
    |        |         |        |
    +--------|         |--------+
    |   6    |         |    2   |
    |        +    +----+        |
    +-------/     |     \-------+
    |   5         |         1   |
    |             |             |
     -------------+-------------

(at the card)

UNKNOWN CONNECTOR at the card.

Pin | Name | Description
--- | --- | ---
1 | VCC | +5 VDC
2 | R/W | Read/Write
3 | CLOCK | Clock
4 | RESET | Reset
5 | GND | Ground
6 | VPP | +21 VDC
7 | I/O | In/Out
8 | FUSE | Fuse

Contributor: Joakim Ögren

Source:
Telecard/Smartcard Technical Spec & Info by Stephane Bausson

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08