# Atari 5200 Cartridge

(at the Atari)

UNKNOWN CONNECTOR at the Atari.

Pin | Name
--- | ---
1 | D0
2 | D1
3 | D2
4 | D3
5 | D4
6 | D5
7 | D6
8 | D7
9 | Enable 80-8F
10 | Enable 40-7F
11 | Not Connected
12 | Ground
13 | Ground
14 | Ground (System Clock 02 on 2 port)
15 | A6
16 | A5
17 | A2
18 | Interlock
19 | A0
20 | A1
21 | A3
22 | A4
23 | Ground
24 | Ground (Video In on 2 port)
25 | Ground
26 | +5 VDC
27 | A7
28 | Not Connected
29 | A8
30 | Audio In (2 port)
31 | A9
32 | A13
33 | A10
34 | A12
35 | A11
36 | Interlock

Contributor: Joakim Ögren

Source:
Classic Atari 2600/5200/7800 Game Systems FAQ

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08