# Spectravideo SVI318/328 Cassette

    +-------------+
    |1 2 3 4 5 6 7|
    +-------------+

(at the computer)

7 PIN FEMALE EDGE CONNECTOR at the computer.

Pin | Name | Description
--- | --- | ---
1 | 12v | Power 100mA
2 | CASR | Cassette data read
3 | CASW | Cassette data write
4 | AUDIO | Cassette audio
5 | GND | System ground
6 | ME |
7 | READY | System Ready

Contributor: Rob Gill

Source:
SVI mk II user manual

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07