# MSX Parallel

(at the Computer)

14 PIN CENTRONICS FEMALE at the Computer.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | /STB |  | Strobe
2 | PDB0 |  | Data 0
3 | PDB1 |  | Data 1
4 | PDB2 |  | Data 2
5 | PDB3 |  | Data 3
6 | PDB4 |  | Data 4
7 | PDB5 |  | Data 5
8 | PDB6 |  | Data 6
9 | PDB7 |  | Data 7
10 | n/c | - |
11 | BUSY |  | Printer is busy
12 | n/c | - |
13 | n/c | - |
14 | GND | - | Signal Ground

Note: Direction is Computer relative Printer.

Contributor: Joakim Ögren

Source:
Mayer's SV738 X'press I/O map

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08