# Video to TV SCART

(to the TV)
(to the Video Recorder)

21 PIN SCART MALE to the TV.
21 PIN SCART MALE to the Video Recorder.

| TV | VCR |
--- | --- | --- | ---
Audio Right Out | 1 | 2 | Audio Right In
Audio Right In | 2 | 1 | Audio Right Out
Audio Left Out | 3 | 6 | Audio Left In
Audio Left In | 6 | 3 | Audio Left Out
Audio Ground | 4 | 4 | Audio Ground
Red | 15 | 15 | Red
Red Ground | 13 | 13 | Red Ground
Green | 11 | 11 | Green
Green Ground | 9 | 9 | Green Ground
Blue | 7 | 7 | Blue
Blue Ground | 5 | 5 | Blue Ground
Status / 16:9 | 8 | 8 | Status / 16:9
Reserved | 10 | 10 | Reserved
Reserved | 12 | 12 | Reserved
Fast Blanking Ground | 14 | 14 | Fast Blanking Ground
Fast Blanking | 16 | 16 | Fast Blanking
Video Out Ground | 17 | 18 | Video In Ground
Video In Ground | 18 | 17 | Video Out Ground
Video Out | 19 | 20 | Video In
Video In | 20 | 19 | Video Out
Ground | 21 | 21 | Ground

Contributor: Joakim Ögren

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07