# Cisco Console Port

Used to configure a Cisco router.

(at the Cisco hub)
(at the cables)

RJ45 FEMALE CONNECTOR at the Cisco routers.
RJ45 MALE CONNECTOR at the cables.

Pin | Name | Description | Dir
--- | --- | --- | ---
1 | RTS | Request To Send |
2 | DTR | Data Terminal Ready |
3 | TXD | Tranceive Data |
4 | n/c | Not connected |
5 | n/c | Not connected |
6 | RXD | Receive Data |
7 | DSR | Data Set Ready |
8 | CTS | Clear To Send |

Contributor: Joakim Ögren, Damien Miller

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07