# GEOCable

(to the C64).
(to the Printer)

DZM 12 DREH to the C64 UserPort.
36 PIN CENTRONICS MALE at the Printer.

| C64 | Printer |
--- | --- | --- | ---
Ground | A | 33 | Ground
Flag 2 | B | 11 | Busy
PB0 | C | 2 | Data 1
PB1 | D | 3 | Data 2
PB2 | E | 4 | Data 3
PB3 | F | 5 | Data 4
PB4 | H | 6 | Data 5
PB5 | J | 7 | Data 6
PB6 | K | 8 | Data 7
PB7 | L | 9 | Data 8
PA2 | M | 1 | Strobe
Ground | N | 16 | Ground

Contributor: Joakim Ögren

Source:
comp.sys.cbm General FAQ v3.1 Part 7

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08