# ATX Aux Power Supply

To be used for motherboards requiring 250W or 300W

(at ???)

6 PIN MOLEX 90331-0010 at ???

Pin | Name |  | Color | Description
--- | --- | --- | --- | ---
1 | COM |  | Black | Ground
2 | COM |  | Black | Ground
3 | COM |  | Black | Ground
4 | 3.3V |  | Orange | +3.3 VDC
5 | 3.3V |  | Orange | +3.3 VDC
6 | 5V |  | Red | +5 VDC

Recommended wiresize 16 AWG

Contributor: Joakim Ögren

Source:
ATX Spec v2.03 at Platform Development Support

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08