# OpenLDI

36 PIN MDR36 FEMALE

Used on SGI digital flat panel monitors.

Standard by VICI
Protocol: LVDS

Pin | Name
--- | ---
1 | Link2 D0-
2 | Link2 DO+
3 | Link2 D1-
4 | Link2 D1+
5 | Link2 D2-
6 | Link2 D2+
7 | NC NC
8 | NC NC
9 | GND GND
10 | GND GND
11 | NC NC
12 | NC NC
13 | Link1 D0-
14 | Link1 D0+
15 | Link1 D1-
16 | Link1 D1+
17 | Link1 D2-
18 | Link1 D2+
19 | Link2 D3-
20 | Link2 D3+
21 | Link2 CLK-
22 | Link2 CLK+
23 | NC NC
24 | NC NC
25 | NC NC
26 | GND GND
27 | NC NC
28 | GND GND
29 | NC NC
30 | NC NC
31 | NC NC
32 | GND GND
33 | Link1 CLK-
34 | Link1 CLK+
35 | Link1 D3-
36 | Link1 D3+

Contributor: Joakim Ögren

Source:
Tech page at Network Technologies Inc

Info: VICI

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07