# Spectravideo SVI318/328 Game Cartridge

(at the computer)

30 PIN FEMALE EDGE at the computer.

Pin | Name
--- | ---
1 | +5v
2 | +5v
3 | A7
4 | A12
5 | A6
6 | A13
7 | A5
8 | A8
9 | A4
10 | A9
11 | A3
12 | A11
13 | A10
14 | A2
15 | A0
16 | A1
17 | D0
18 | D7
19 | D1
20 | D6
21 | D2
22 | D5
23 | D3
24 | D4
25 | CCS3
26 | CCS4
27 | CCS1
28 | CCS2
29 | GND
30 | GND

Contributor: Rob Gill

Source:
SVI 328 mk II user manual

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07