# TG-16 Cartridge

Available on the TG-16.

(at the TG-16)

UNKNOWN CONNECTOR at the TG-16.

Pin | Name | Description
--- | --- | ---
1 | ? |
2 | ? |
3 | A18? | Address 18
4 | A16 | Address 16
5 | A15 | Address 15
6 | A12 | Address 12
7 | A7 | Address 7
8 | A6 | Address 6
9 | A5 | Address 5
10 | A4 | Address 4
11 | A3 | Address 3
12 | A2 | Address 2
13 | A1 | Address 1
14 | A0 | Address 0
15 | D7 | Data 7
16 | D6 | Data 6
17 | D5 | Data 5
18 | GND | Ground
19 | D4 | Data 4
20 | D3 | Data 3
21 | D2 | Data 2
22 | D1 | Data 1
23 | D0 | Data 0
24 | /CE | Chip Select
25 | A10 | Address 10
26 | /OE | Output Enable
27 | A11 | Address 11
28 | A9 | Address 9
29 | A8 | Address 8
30 | A13 | Address 13
31 | A14 | Address 14
32 | A17 | Address 17
33 | A19? | Address 19
34 | R/W | Read/Write
35 | ? |
36 | ? |
37 | ? |
38 | +5V | +5 VDC

Pin 1 is the short pin on the left (if the card is to inserted forwards)
Pin 38 is the long pin on the right.

Contributor: Joakim Ögren

Source:
Video Games FAQ (Part 3) - Pinout by David Shadoff

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08