# LapLink/InterLink Parallel

Will work with:

- LapLink from Travelling Software
- MS-DOS v6.0 InterLink from Microsoft
- Windows 95 Direct Cable connection from Microsoft
- Norton Commander v4.0 & v5.0 from Symantec

(To Computer 1).
(To Computer 2).

25 PIN D-SUB MALE to Computer 1.
25 PIN D-SUB MALE to Computer 2.

Name | Pin | Pin | Name
--- | --- | --- | ---
Data Bit 0 | 2 | 15 | Error
Data Bit 1 | 3 | 13 | Select
Data Bit 2 | 4 | 12 | Paper Out
Data Bit 3 | 5 | 10 | Acknowledge
Data Bit 4 | 6 | 11 | Busy
Acknowledge | 10 | 5 | Data Bit 3
Busy | 11 | 6 | Data Bit 4
Paper Out | 12 | 4 | Data Bit 2
Select | 13 | 3 | Data Bit 1
Error | 15 | 2 | Data Bit 0
Reset | 16 | 16 | Reset
Select | 17 | 17 | Select
Signal Ground | 25 | 25 | Signal Ground

Contributor: Joakim Ögren

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07