# Panasonic CD-ROM

(at the controller & CD-ROM)
(at the cable.)

40 PIN IDC MALE at the controller & CD-ROM.
40 PIN IDC FEMALE at the cable.

Pin | Name | Description
--- | --- | ---
1 | GND | Ground
2 | RESET | CD-Reset
3 | GND | Ground
4 | GND | Ground
5 | GND | Ground
6 | MODE0 | Operation Mode Bit 0
7 | GND | Ground
8 | MODE1 | Operation Mode Bit 1
9 | GND | Ground
10 | WRITE | CD-Write
11 | GND | Ground
12 | READ | CD-Read
13 | GND | Ground
14 | ST0 | CD-Status Bit 0
15 | GND | Ground
16 | n/c | No Connection
17 | GND | Ground
18 | n/c | No Connection
19 | GND | Ground
20 | ST1 | CD-Status Bit 1
21 | GND | Ground
22 | EN | CD-Data Enable
23 | GND | Ground
24 | ST2 | CD-Status Bit 2
25 | GND | Ground
26 | S/DE | CD-Status/Data Enable
27 | GND | Ground
28 | ST3 | CD-Status Bit 3
29 | GND | ground
30 | GND | ground
31 | D7 | CD-Data 7
32 | D6 | CD-Data 6
33 | GND | ground
34 | D5 | CD-Data 5
35 | D4 | CD-Data 4
36 | D3 | CD-Data 3
37 | GND | ground
38 | D2 | CD-Data 2
39 | D1 | CD-Data 1
40 | D0 | CD-Data 0

Contributor: Keith Solomon

Source:
SoundFX 16-bit Multimedia Kit Hardware Manual from Reveal

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07