# Apple AudioVision

45 PIN UNKNOWN CONNECTOR ??

Pin | Name
--- | ---
1 | Analog audio ground
2 | Audio input shield
3 | Left channel audio input
4 | Right channel audio input
5 | Left channel audio output
6 | Right channel audio output
7 | Reserved
8 | Monitor ID sense line 1
9 | Monitor ID sense line 2
10 | Green ground (shield)
11 | Green video output (75 )
12 | Video input power ground
13 | Power for camera +5 V
14 | Reserved
15 | Reserved
16 | Reserved
17 | Reserved
18 | Monitor ID sense line 3
19 | S-video input shield
20 | S-video input luminance (Y)
21 | S-video input chroma (C)
22 | Reserved
24 | Reserved
25 | Reserved
26 | Red ground (shield)
27 | Red video output (75 )
28 | I2C data signal
29 | I2C clock signal
30 | Reserved
31 | Monitor ID
32 | Monitor ID
33 | Vertical sync signal
34 | Composite sync signal
35 | ADB power +5 V
36 | ADB ground
37 | ADB data
38 | Keyboard switch
39 | Reserved
40 | Reserved
41 | Monitor ID
42 | Horizontal sync signal
43 | Video sync ground
44 | Blue ground (shield)
45 | Blue video output (75 )

Contributor: Joakim Ögren

Source:
Apple Tech Info Library 14703: Power Macintosh Pinouts at Apple TIL homepage
Apple Tech Info Library 12719: AudioVision 14 Display High-Density Connector Pinouts at Apple TIL homepage

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2000-07-08