# SCSI Cable (D-Sub to Hi D-Sub)

(to the Amiga/Mac).
(To the peripheral).

25 PIN D-SUB MALE to the Amiga/Mac.
50 PIN HI-DENSITY D-SUB MALE to the peripheral.

| DSub | Hi DSub
--- | --- | ---
Request | 1 | 49
Message | 2 | 46
Input/Output | 3 | 50
Reset | 4 | 45
Acknowledge | 5 | 44
Busy | 6 | 43
Data Bus 0 | 8 | 26
Data Bus 3 | 10 | 29
Data Bus 5 | 11 | 31
Data Bus 6 | 12 | 32
Data Bus 7 | 13 | 33
Control/Data | 15 | 48
Attention | 17 | 41
Select | 19 | 47
Data Parity | 20 | 34
Data Bus 1 | 21 | 27
Data Bus 2 | 22 | 28
Data Bus 4 | 23 | 30
Termination Power | 25 | 38

Note: All the other pins (7+9+14+16+18+24) at the DSub should be connected to pins 1-25 at the Hi-density D-Sub connector.

Contributor: Joakim Ögren

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07