# MSX Cassette

(at the computer)
(at the cassette cable)

8 PIN DIN (DIN45326) FEMALE at the computer.
8 PIN DIN (DIN45326) MALE at the cassette cable.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | GND |  | Ground
2 | GND |  | Ground
3 | GND |  | Ground
4 | CMTOUT |  | Sound Output
5 | CMTIN |  | Sound Input
6 | REM+ |  | Remote control (from relay)
7 | REM- |  | Remote control (from relay)
8 | GND |  | Ground

Note: Direction is Computer relative Cassette.

Contributor: Joakim Ögren

Source:
Mayer's SV738 X'press I/O map

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08