# Parallel (PC)

(at the PC)

25 PIN D-SUB FEMALE at the PC.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | /STROBE |  | Strobe
2 | D0 |  | Data Bit 0
3 | D1 |  | Data Bit 1
4 | D2 |  | Data Bit 2
5 | D3 |  | Data Bit 3
6 | D4 |  | Data Bit 4
7 | D5 |  | Data Bit 5
8 | D6 |  | Data Bit 6
9 | D7 |  | Data Bit 7
10 | /ACK |  | Acknowledge
11 | BUSY |  | Busy
12 | PE |  | Paper End
13 | SEL |  | Select
14 | /AUTOFD |  | Autofeed
15 | /ERROR |  | Error
16 | /INIT |  | Initialize
17 | /SELIN |  | Select In
18 | GND |  | Signal Ground
19 | GND |  | Signal Ground
20 | GND |  | Signal Ground
21 | GND |  | Signal Ground
22 | GND |  | Signal Ground
23 | GND |  | Signal Ground
24 | GND |  | Signal Ground
25 | GND |  | Signal Ground

Note: Direction is Computer relative Device.

Contributor: Joakim Ögren, Petr Krc

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07