# SUN SROMBOlite

Available on SUN SPARCengine motherboards
Seems to be for SUN internal factory tests/programming

28 PIN IDC MALE at the motherboard

Pin | Name
--- | ---
1 | +5V
2 | GND
3 | EB_RD_L
4 | EB_WR_L
5 | EB_SCC_CS_L
6 | EB_LATCH
7 | EB_RDY_L
8 | EB_DAT<0>
9 | EB_DAT<1>
10 | EB_DAT<2>
11 | EB_DAT<3>
12 | BRST_L
13 | EB_DAT<4>
14 | EB_DAT<5>
15 | EB_DAT<6>
16 | EB_DAT<7>
17 | ROMBO_CS_L
18 | EB_ADR<0>
19 | EB_ADR<1>
20 | EB_ADR<2>
21 | EB_ADR<3>
22 | SYNC_SER_IRQ_L
23 | EB_ADR<4>
24 | EB_ADR<5>
25 | EB_ADR<6>
26 | EB_ADR<7>
27 | +5V
28 | GND

Contributor: Joakim Ögren

Source:
SUN SPARCengine CP 1500 Manual

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07