# Apple Video Mirror

Available on Apple Power Macintosh 5400
Fullname: Optional Video Display Mirror Output Feature

22 PIN UNKNOWN CONNECTOR

Pin | Name | Description
--- | --- | ---
1 | VID.GND | Video ground
2 | RED | Red signal
3 | GREEN | Green signal
4 | VID.GND | Video ground
5 | VID.GND | Video ground
6 | BLUE | Blue signal
7 | CSYNC | C sync
8 | VSYNC | Vertical sync
9 | MLB.SYNC.EN.L | Not used (reserved)
10 | HSYNC | Horizontal sync
11 | DAC.ISET.1 | Not used(reserved)
12 | DAC.ISET.2 | Not used (reserved)
13 | SND.GND | Not used (reserved)
14 | SND.RIGHT | Not used (reserved)
15 | SND.LEFT | Not used (reserved)
16 | +5V | +5 volts
17 | GND | Ground
18 | SDAT | Not used (reserved)
19 | SCLK | Not used (reserved)
20 | +12V | +12 volts
21 | -12V | -12 volts
22 | Dot | Clock Scaled dot clock (scaled to 10 percent)

Contributor: Joakim Ögren

Source:
Apple Power Macintosh 5400 Developer Note

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07