# SmartCard ISO 7816-2

     -------------+-------------
    |   1         |         5   |
    |             |             |
    +-------\     |     /-------+
    |   2    +----+    +    6   |
    |        |         |        |
    +--------|         |--------+
    |   3    |         |    7   |
    |        +----+----+        |
    +-------/     |     \-------+
    |   4         |         8   |
    |             |             |
     -------------+-------------

(at the card)

UNKNOWN CONNECTOR at the card.

Pin | Name | Description
--- | --- | ---
1 | VCC | +5 VDC
2 | RESET | Reset
3 | CLOCK | Clock
4 | n/c | Not connected
5 | GND | Ground
6 | n/c | Not connected
7 | I/O | In/Out
8 | n/c | Not connected

Contributor: Joakim Ögren

Source:
Telecard/Smartcard Technical Spec & Info by Stephane Bausson

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08