# Operation Amplifier: Addition

VOUT= -(V1/R1+V2/R2)*RO

This circuit is used to add several signals to one. By setting all resistors to the same value, R1=R2=RO, you get the following formula:

VOUT= -(V1+V2)

You can theoretically add how many signals you like. Here's an example with three in-signals:

VOUT= -(V1/R1+V2/R2+V3/R3)*RO

Contributor: Joakim Ögren

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07