# PCMCIA

PCMCIA=Personal Computer Memory Card International Association.

(at the controller)
(at the peripherals)

68 PIN ??? MALE at the controller.
68 PIN ??? FEMALE at the peripherals.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | GND |  | Ground
2 | D3 |  | Data 3
3 | D4 |  | Data 4
4 | D5 |  | Data 5
5 | D6 |  | Data 6
6 | D7 |  | Data 7
7 | /CE1 |  | Card Enable 1
8 | A10 |  | Address 10
9 | /OE |  | Output Enable
10 | A11 |  | Address 11
11 | A9 |  | Address 9
12 | A8 |  | Address 8
13 | A13 |  | Address 13
14 | A14 |  | Address 14
15 | /WE:/P |  | Write Enable : Program
16 | /READY:/IREQ |  | Ready : Busy (IREQ)
17 | VCC |  | +5V
18 | VPP1 |  | Programming Voltage (EPROM)
19 | A16 |  | Address 16
20 | A15 |  | Address 15
21 | A12 |  | Address 12
22 | A7 |  | Address 7
23 | A6 |  | Address 6
24 | A5 |  | Address 5
25 | A4 |  | Address 4
26 | A3 |  | Address 3
27 | A2 |  | Address 2
28 | A1 |  | Address 1
29 | A0 |  | Address 0
30 | D0 |  | Data 0
31 | D1 |  | Data 1
32 | D2 |  | Data 2
33 | /WP:/IOIS16 |  | Write Protect : IOIS16
34 | GND |  | Ground
35 | GND |  | Ground
36 | /CD1 |  | Card Detect 1
37 | D11 |  | Data 11
38 | D12 |  | Data 12
39 | D13 |  | Data 13
40 | D14 |  | Data 14
41 | D15 |  | Data 15
42 | /CE2 |  | Card Enable 2
43 | /VS1 |  | Refresh
44 | /IORD | ? | I/O Read
45 | /IOWR | ? | I/O Write
46 | A17 |  | Address 17
47 | A18 |  | Address 18
48 | A19 |  | Address 19
49 | A20 |  | Address 20
50 | A21 |  | Address 21
51 | VCC |  | +5V
52 | VPP2 |  | Programming Voltage 2 (EPROM)
53 | A22 |  | Address 22
54 | A23 |  | Address 23
55 | A24 |  | Address 24
56 | A25 |  | Address 25
57 | /VS2 | ? | RFU
58 | RESET | ? | RESET
59 | /WAIT | ? | WAIT
60 | /INPACK | ? |
61 | /REG |  | Register Select
62 | /BVD2:SPKR |  | Battery Voltage Detect 2 : SPKR
63 | /BVD1:STSCHG |  | Battery Voltage Detect 1 : STSCHG
64 | D8 |  | Data 8
65 | D9 |  | Data 9
66 | D10 |  | Data 10
67 | /CD2 |  | Card Detect 2
68 | GND |  | Ground

Note: Direction is Controller (computer) relative PCMCIA-card.

Contributor: Joakim Ögren, Karsten Wenke

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07