# Digital Flat Panel (DFP)

MDR20 female

Used on digital flat panel monitors.

Standard by DFP Group
Protocol: PanelLink

Pin | Name
--- | ---
1 | TX1+
2 | TX1-
3 | SHLD1
4 | SHLDC
5 | TXC+
6 | TXC-
7 | GND
8 | +5V
9 | NC
10 | NC
11 | TX2+
12 | TX2-
13 | SHLD2
14 | SHLD0
15 | TX0+
16 | TX0-
17 | NC
18 | HPD
19 | DDC_DAT
20 | DDC_CLK

Contributor: Joakim Ögren

Source:
Tech page at Network Technologies Inc

Info: DFP Group

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07