# AUI

Is the directions right???

(at the Ethernet card)

15 PIN D-SUB FEMALE at the Ethernet card.

Pin | Description
--- | ---
1 | control in circuit shield
2 | control in circuit A
3 | data out circuit A
4 | data in circuit shield
5 | data in circuit A
6 | voltage common
7 | ?
8 | control out circuit shield
9 | control in circuit B
10 | data out circuit B
11 | data out circuit shield
12 | data in circuit B
13 | voltage plus
14 | voltage shield
15 | ?

Contributor: Joakim Ögren

Source:
Tommy's pinout Collection by Tommy Johnson

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07