# ECL

(at the videocard)
(at the monitor cable)

9 PIN D-SUB FEMALE at the videocard.
9 PIN D-SUB MALE at the monitor cable.

Pin | Name | Description
--- | --- | ---
1 | ECL | ECL?
2 | ECLGND | ECL Video Ground
3 | HSYNC | Horizontal Sync
4 | VSYNC | Vertical Sync
5 | +5V | +5 VDC
6 | ECLGND | ECL Video Ground
7 | ECLGND | ECL Video Ground
8 | SYNCGND | Sync Ground
9 | +5GND | Ground (for +5V)

Contributor: Joakim Ögren

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07