# Floppy

The original floppy cable required that each drive was jumpered to the right ID. But IBM come up with an idea to avoid jumpering the floppies.
If wire 10-16 are twisted before the last connector the jumpering is avoided. Each drive should be jumpered to act as Drive 2. If only one drive is used then leave the middle connector free.
The IDC could also be an edge connector on some old drives.

    Controller           Drive 2   Twist   Drive 1
    +--+                   +--+            +--+
    |::|===================|  |============|  |  <-Pin 1
    |::|===================|  |=====\/=====|  |
    |::|===================|  |=====/\=====|  |
    |::|===================|  |============|  |
    |::|===================|  |============|  |
    |::|===================|  |============|  |
    |::|===================|  |============|  |
    +--+                   +--+            +--+

(to the Controller)
(to the Drive 2)
(to the Drive 1)

34 PIN IDC FEMALE to the Controller.
34 PIN IDC FEMALE to the Drive 2.
34 PIN IDC FEMALE to the Drive 1.

| Controller | Drive 1 | Drive 2
--- | --- | --- | ---
Wire 1-9 | 1-9 | 1-9 | 1-9
Wire 10 | 10 | 16 | 10
Wire 11 | 11 | 15 | 11
Wire 12 | 12 | 14 | 12
Wire 13 | 13 | 13 | 13
Wire 14 | 14 | 12 | 14
Wire 15 | 15 | 11 | 15
Wire 16 | 16 | 10 | 16
Wire 17-34 | 17-34 | 17-34 | 17-34

Contributor: Joakim Ögren

Source:
TheRef TechTalk

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08