# ZX Spectrum 128 RGB

Can be found at the Sinclair ZX Spectrum 128.

(at the computer)
(at the monitor cable)

8 PIN DIN (DIN45326) FEMALE at the computer.
8 PIN DIN (DIN45326) MALE at the monitor cable.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | CVBS |  | Composite Video (PAL, 75 ohms, 1.2V p-p)
2 | GND |  | Ground
3 | BOUT |  | Bright Output
4 | CSYNC |  | Composite Sync
5 | VSYNC |  | Vertical Sync
6 | G |  | Green
7 | R |  | Red
8 | B |  | Blue

Note: Direction is Computer relative Monitor.

Contributor: Joakim Ögren

Source:
Online ZX Spectrum 128 Manual Page 3

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08