# C128/C64C to CBM 1902A Monitor

(at the Computer)
(at the Monitor)

8 PIN DIN (DIN45326) MALE at the Computer.
6 PIN DIN MALE at the Monitor.

| Computer | C1902A |
--- | --- | --- | ---
LUM | 1 | 6 | LUM
CHROMA | 8 | 4 | CHROMA
GND | 2 | 3 | GND
AOUT | 3 | 2 | AUDIO

Contributor: Joakim Ögren

Source:
cbm.comp.sys General FAQ v3.1 Part 7

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08