# Modem (9-15)

This cable should be used to connect an internal 14.4kbps Speedster modem to a computer.

(To Computer).
(at the modem)

9 PIN D-SUB FEMALE to the Computer
15 PIN FEMALE ??? to the modem.

| 9 pin | 15 pin | Dir
--- | --- | --- | ---
Carrier Detect | 1 | 11 |
Receive Data | 2 | 13 |
Transmit Data | 3 | 12 |
Data Terminal Ready | 4 | 10 |
System Ground | 5 | 1+8+15 |
Data Set Ready | 6 | 3 |
Request to Send | 7 | 4 |
Clear to Send | 8 | 5 |
Ring Indicator | 9 | 6 |

Contributor: Joakim Ögren, Joerg Brinkel

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08