# Amiga Video

(at the Amiga)

23 PIN D-SUB MALE at the Amiga.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | /XCLK |  | Extern Clock
2 | /XCLKEN |  | Extern Clock Enable (47 Ohm)
3 | RED |  | Analog Red (75 Ohm)
4 | GREEN |  | Analog Green (75 Ohm)
5 | BLUE |  | Analog Blue (75 Ohm)
6 | DI |  | Digital Intensity (47 Ohm)
7 | DR |  | Digital Red (47 Ohm)
8 | DG |  | Digital Green (47 Ohm)
9 | DB |  | Digital Blue (47 Ohm)
10 | /CSYNC |  | Composite Sync (47 Ohm)
11 | /HSYNC |  | Horizontal Sync (47 Ohm)
12 | /VSYNC |  | Vertical Sync (47 Ohm)
13 | GNDRTN |  | Digital Ground (for /XCLKEN) Don't connect with pin 16-20.
14 | /PIXELSW |  | Genlock overlay (47 Ohm)
15 | /C1 |  | Clock out (47 Ohm)
16 | GND |  | Video Ground
17 | GND |  | Video Ground
18 | GND |  | Video Ground
19 | GND |  | Video Ground
20 | GND |  | Video Ground
21 | -12V |  | -12 Volts DC (10 mA max) (A500/A600/A1200)
| -5V |  | -5 Volts DC (10 mA max) (A1000/A2000/A3000/A4000)
22 | +12V |  | +12 Volts DC (100 mA max)
23 | +5V |  | +5 Volts DC (100 mA max)

Note: Direction is Computer relative Monitor.

Contributor: Joakim Ögren

Source:
Amiga 4000 User's Guide from Commodore

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2000-05-28