# SUN AUI

26 PIN HI-DENSITY D-SUB FEMALE at the motherboard.
26 PIN HI-DENSITY D-SUB MALE at the cable.

Available on the SUN SPARCengine 5 motherboard

Pin | Name
--- | ---
1 | Transmit -
2 | Receive +
3 | Collision -
4 | AUI Power
5 | N/C
6 | N/C
7 | N/C
8 | N/C
9 | N/C
10 | N/C
11 | N/C
12 | N/C
13 | N/C
14 | Transmit +
15 | Receive -
16 | Collision +
17 | Ground
18 | N/C
19 | N/C
20 | N/C
21 | N/C
22 | N/C
23 | Ground
24 | Ground
25 | N/C
26 | Ground

Contributor: Joakim Ögren

Source:
SUN SPARCengine 5 manual at SUN manuals site

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07