# EGA

EGA=Enhanced Graphics Adapter.
Videotype: TTL, 16/64 colors.

(at the videocard)
(at the monitor cable)

9 PIN D-SUB FEMALE at the videocard.
9 PIN D-SUB MALE at the monitor cable.

Pin | Name | Description
--- | --- | ---
1 | GND | Ground
2 | SR | Secondary Red
3 | PR | Primary Red
4 | PG | Primary Green
5 | PB | Primary Blue
6 | SG/I | Secondary Green / Intensity
7 | SB | Secondary Blue
8 | H | Horizontal Sync
9 | V | Vertical Sync

Contributor: Joakim Ögren

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07