# IEEE488

12 PIN UNKNOWN CONNECTOR at the Computer

          1  2  3  4  5  6
          =  =  =  =  =  =
         ###### ###########    (At the computer)
          =  =  =  =  =  =
          A  B  C  D  E  F

Pin | Description
--- | ---
A or 1 | GND
B or 2 | +5v
C or 3 | Motor (computer controlled +6v for datasette motor)
D or 4 | Read line from casette
E or 5 | Write line cassette
F or 6 | Cassette Switch Sense (monitors cassette play/ff/rew buttons)

Contributor: Joakim Ögren

Source:
Commodore PET FAQ

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2000-07-07