# Parallel (Amiga 1000)

(at the Amiga 1000)

25 PIN D-SUB MALE at the Amiga 1000.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | /STROBE |  | Strobe
2 | D0 |  | Data Bit 0
3 | D1 |  | Data Bit 1
4 | D2 |  | Data Bit 2
5 | D3 |  | Data Bit 3
6 | D4 |  | Data Bit 4
7 | D5 |  | Data Bit 5
8 | D6 |  | Data Bit 6
9 | D7 |  | Data Bit 7
10 | /ACK |  | Acknowledge
11 | BUSY |  | Busy
12 | POUT |  | Paper Out
13 | SEL |  | Select (Shared with RS232 RING-indicator)
14 | GND |  | Signal Ground
15 | GND |  | Signal Ground
16 | GND |  | Signal Ground
17 | GND |  | Signal Ground
18 | GND |  | Signal Ground
19 | GND |  | Signal Ground
20 | GND |  | Signal Ground
21 | GND |  | Signal Ground
22 | GND |  | Signal Ground
23 | +5V |  | +5 Volts DC (10 mA max)
24 | n/c | - | Not connected.
25 | /RESET |  | Reset

Note: Direction is Computer relative Peripheral.

Contributor: Joakim Ögren

Source:
Amiga 4000 User's Guide from Commodore

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07