# N64 Video

Available on the Nintendo N64.

(at the SNES)
(at the video cable)

SNES A/V MALE CONNECTOR at the SNES.
SNES A/V FEMALE CONNECTOR at the video cable.

Pin | Name | Description
--- | --- | ---
1 | n/c | Not connected
2 | n/c | Not connected
3 | n/c | Not connected
4 | n/c | Not connected
5 | GND | Ground
6 | GND | Ground
7 | Y | S-Video Y
8 | C | S-Video C
9 | CVBS | Composite Video
10 | +5V | +5 VDC
11 | L+R | Left+Right Audio (Mono)
12 | L-R | Left-Right Audio (Used to calculate Stereo)

Contributor: Joakim Ögren

Source:
Video Games FAQ (Part 3)
Pinout from Radio Electronics April 1992
SNES A/V Pinout at GamesX

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07