# Enhanced Video Connector (EVC)

Defined by Video Electronic Standards Association (VESA)

(at the motherboard)
(at the cable)

35 PIN MOLEX "MicroCross" FEMALE at the videocard/monitor
35 PIN MOLEX "MicroCross" MALE at the cable

Pin | Name
--- | ---
1 | Audio output, Right
2 | Audio output, Left
3 | Audio output return
4 | Sync return
5 | Horizontal sync (TTL)
6 | Vertical sync (TTL)
7 | Reserved
8 | Reserved
9 | 1394 pair A, data -
10 | 1394 pair A, data +
11 | Reserved
12 | Reserved
13 | Video input, Y or composite in
14 | Video input, return
15 | Video input, C in
16 | USB data +
17 | USB data -
18 | USB/1394 common mode shield
19 | 1394 Vg
20 | 1394 Vp
21 | Audio input, Left
22 | Audio input, Right
23 | Audio input return
24 | Stereo sync (TTL)
25 | DDC return
26 | DDC data (SDA)
27 | DDC, clock (SCL)
28 | +5 VDC
29 | 1394 pair B, clock +
30 | 1394 pair B, clock -
C1 | Red Video
C2 | Green Video
C3 |
C4 | Blue Video
C5 | Ground

Contributor: Joakim Ögren

Source:
Tech page at Network Technologies Inc

Info:
Video Electronic Standards Association (VESA)

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07