# Keyboard (Amiga CD32)

The Amiga CD32 keyboard connector also includes a serialport.

(at the computer)

6 PIN MINI-DIN FEMALE (PS/2 STYLE) at the computer.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | /DATA |  | Data
2 | /TxD |  | Transmit Data (0-5V and reversed)
3 | GND |  | Ground
4 | +5V |  | +5 Volts DC (100 mA max)
5 | CLOCK |  | Clock
6 | /RxD |  | Receive Data (0-5V and reversed)

Note: Direction is Computer relative Keyboard.

Contributor: Joakim Ögren, Dirk Duesterberg

Source:
CD32 keyboard port info, Usenet posting by Klaus Hegemann

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07