# SNES Cartridge

Available on the Nintendo SNES.

    +-------------------------------//----------------------------+
    | 32 33 34 35 | 36 37 38 39 40 //53 55 56 57 58 | 59 60 61 62 |
    | 01 02 03 04 | 05 06 07 08 09// 22 24 25 26 27 | 28 29 30 31 |
    +----------------------------//-------------------------------+

(at the SNES)

UNKNOWN CONNECTOR at the SNES.

Pin | Name | Description
--- | --- | ---
1 |  |
2 |  |
3 |  |
4 |  |
5 | GND | Ground
6 | A11 | Address 11
7 | A10 | Address 10
8 | A9 | Address 9
9 | A8 | Address 8
10 | A7 | Address 7
11 | A6 | Address 6
12 | A5 | Address 5
13 | A4 | Address 4
14 | A3 | Address 3
15 | A2 | Address 2
16 | A1 | Address 1
17 | A0 | Address 0
18 | /IRQ | Interrupt
19 | D0 | Data 0
20 | D1 | Data 1
21 | D2 | Data 2
22 | D3 | Data 3
23 | /READ | Read
24 | CIC | ?
25 | CIC | ?
26 | /RAM ENABLE | RAM Enable
27 | VCC | +5 VDC
28 |  |
29 |  |
30 |  |
31 |  |
32 |  |
33 |  |
34 |  |
35 |  |
36 | GND | Ground
37 | A12 | Address 12
38 | A13 | Address 13
39 | A14 | Address 14
40 | A15 | Address 15
41 | A16 | Address 16
42 | A17 | Address 17
43 | A18 | Address 18
44 | A19 | Address 19
45 | A20 | Address 20
46 | A21 | Address 21
47 | A22 | Address 22
48 | A23 | Address 23
49 | /ROM ENABLE | ROM Enable
50 | D4 | Data 4
51 | D5 | Data 5
52 | D6 | Data 6
53 | D7 | Data 7
54 | /WRITE | Write
55 | CIC | ?
56 | CIC | ?
57 | n/c | Not connected
58 | VCC | +5 VDC
59 |  |
60 |  |
61 |  |
62 |  |

Contributor: Joakim Ögren

Source:
Video Games FAQ (Part 3) - Pinout by Thomas Rolfes

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08