# Plug and Display Digital (P&D-D)

Defined by Video Electronic Standards Association (VESA) in the Plug and Display (P&D) standard

(at the motherboard)
(at the cable)

30 PIN MOLEX "MicroCross" FEMALE at the videocard/monitor
30 PIN MOLEX "MicroCross" MALE at the cable

Pin | Name
--- | ---
1 | TMDS Data 2 +
2 | TMDS Data 2 -
3 | TMDS Data return
4 | Unused
5 | Unused
6 | Unused
7 | TMDS Clock return
8 | Charge power (optional)
9 | 1394 pair A, data -
10 | 1394 pair A, data +
11 | TMDS Data 1 +
12 | TMDS Data 1 -
13 | TMDS Data 1 return
14 | TMDS Clock +
15 | TMDS Clock -
16 | USB data +
17 | USB data -
18 | 1394 outer shield (optional) & Charge Power return
19 | 1394 Vg
20 | 1394 Vp
21 | TMDS Data 0 +
22 | TMDS Data 0 -
23 | TMDS Data 0 return
24 | Unused
25 | DDC return
26 | DDC data (SDA)
27 | DDC clock (SCL)
28 | +5 VDC
29 | 1394 pair B, clock +
30 | 1394 pair B, clock -

Contributor: Joakim Ögren

Source:
Tech page at Network Technologies Inc

Info:
Video Electronic Standards Association (VESA)

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08