# Sega Dreamcast A/V

Pin | Description
--- | ---
1 | Ground
2 | Right Audio
3 | Left Audio
4 | +12v
5 | +5v
6 | 31 kHz RGB - (VGA rate) Connect to GND with pin 7
7 | 15 kHz RGB - (TV rate) Connect to GND
8 | Vertical Sync (for VGA)
9 | Horizontal Sync (for VGA)
10 | Composite Sync
11 | S-video
12 | S-video
13 | Composite Video
14 | Blue (Use 220uf cap)
15 | Green (Use 220uf cap)
16 | Red (use 220uf cap)

Contributor: Joakim Ögren, Marcus Hilbe, Marvin

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2000-07-11