# MIDI

(to the 1st peripheral)
(to the 2nd peripheral)

5 PIN DIN 180° (DIN41524) MALE to the 1st peripheral.
5 PIN DIN 180° (DIN41524) MALE to the 1st peripheral.

| 1st | 2nd
--- | --- | ---
Shield | 2 | 2
Current Source | 4 | 4
Current Sink | 5 | 5

Note: Although that pin 2 only is connected at MIDI Out it's simpler to connect it to both ends.

Contributor: Joakim Ögren

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07