# Amstrad CPC6128 Printer Port

(at the computer)

34 PIN FEMALE EDGE at the computer.

Pin | Name | Description
--- | --- | ---
1 | /STROBE | Strobe
2 | D0 | Data 0
3 | D1 | Data 1
4 | D2 | Data 2
5 | D3 | Data 3
6 | D4 | Data 4
7 | D5 | Data 5
8 | D6 | Data 6
9 | GND | Ground
10 | n/c | Not connected
11 | BUSY | Busy
12 | n/c | Not connected
13 | n/c | Not connected
14 | GND | Ground
15 | n/c | Not connected
16 | n/c | Not connected
17 | n/c | Not connected
16 | GND | Ground
17 | n/c | Not connected
19 | GND | Ground
20 | GND | Ground
21 | GND | Ground
22 | GND | Ground
23 | GND | Ground
24 | GND | Ground
25 | GND | Ground
26 | GND | Ground
27 | n/c | Not connected
28 | GND | Ground
29 | n/c | Not connected
30 | n/c | Not connected
31 | n/c | Not connected
32 | n/c | Not connected
33 | GND | Ground
34 | n/c | Not connected
35 | n/c | Not connected

Note: Pin 18 does not exist

Contributor: Joakim Ögren, Agnello Guarracino

Source:
Amstrad CPC6128 User Instructions Manual

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07