# Plug and Display Analog/Digital (P&D-A/D)

Defined by Video Electronic Standards Association (VESA) in the Plug and Display (P&D) standard

(at the motherboard)
(at the cable)

35 PIN MOLEX "MicroCross" FEMALE at the videocard/monitor
35 PIN MOLEX "MicroCross" MALE at the cable

Pin | Name
--- | ---
1 | TMDS Data 2 +
2 | TMDS Data 2 -
3 | TMDS Data return
4 | Hz and Vt Sync return
5 | Horizontal sync/Composite sync
6 | Vertical sync
7 | TMDS Clock return
8 | Charge power
9 | 1394 pair A, data -
10 | 1394 pair A, data +
11 | TMDS Data 1 +
12 | TMDS Data 1 -
13 | TMDS Data 1 return
14 | TMDS Clock +
15 | TMDS Clock -
16 | USB data +
17 | USB data -
18* | 1394 outer shield (optional) & Charge Power return
19 | 1394 Vg
20 | 1394 Vp
21 | TMDS Data 0 +
22 | TMDS Data 0 -
23 | TMDS Data 0 return
24 | Stereo sync (TTL)
25 | DDC return & Stereo Sync return
26 | DDC data (SDA)
27 | DDC clock (SCL)
28 | +5 VDC
29 | 1394 pair B, clock +
30 | 1394 pair B, clock -
C1 | Red Video
C2 | Green Video
C3 | Pixel clock (optional)
C4 | Blue Video
C5 | Video / Pixel Clock Ground

Contributor: Joakim Ögren

Source:
Tech page at Network Technologies Inc

Info:
Video Electronic Standards Association (VESA)

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08