# Serial (SGI MiniDIN)

(at the computer)

8 PIN MINI-DIN (CENTER PIN) FEMALE at the computer.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | DTR |  | Data Terminal Ready
2 | CTS |  | Clear to Send
3 | TXD |  | Transmit Data
4 | GND |  | System Ground
5 | RXD |  | Receive Data
6 | RTS |  | Request to Send
7 | CD |  | Carrier Detect
8 | GND |  | System Ground

Note: Direction is DTE (Computer) relative DCE (Modem).

Contributor: Egon Kastelijn

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07