# Printer

(to the Computer)
(to the Printer)

25 PIN D-SUB MALE to the Computer
36 PIN CENTRONICS MALE to the Printer.

| 25-DSub | 36-Cen
--- | --- | ---
Strobe | 1 | 1
Data Bit 0 | 2 | 2
Data Bit 1 | 3 | 3
Data Bit 2 | 4 | 4
Data Bit 3 | 5 | 5
Data Bit 4 | 6 | 6
Data Bit 5 | 7 | 7
Data Bit 6 | 8 | 8
Data Bit 7 | 9 | 9
Acknowledge | 10 | 10
Busy | 11 | 11
Paper Out | 12 | 12
Select | 13 | 13
Autofeed | 14 | 14
Error | 15 | 32
Reset | 16 | 31
Select | 17 | 36
Signal Ground | 18 | 33
Signal Ground | 19 | 19,20
Signal Ground | 20 | 21,22
Signal Ground | 21 | 23,24
Signal Ground | 22 | 25,26
Signal Ground | 23 | 27
Signal Ground | 24 | 28,29
Signal Ground | 25 | 30,16
Shield | Shield | Shield+17

Contributor: Joakim Ögren, Petr Krc

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07