# Conrad Electronics MM3610D (9)

Use this cable to connect a Conrad Electronics Multimeter 3610D to a PC:s serialport.

(To PC).
(To multimeter).

9 PIN D-SUB FEMALE to PC.
5 PIN UNKNOWN CONNECTOR to the multimeter

| PC | Conrad | Dir
--- | --- | --- | ---
Request To Send | 7 | 1 |
Receive Data | 2 | 2 |
Transmit Data | 3 | 3 |
Data Terminal Ready | 4 | 4 |
Ground | 5 | 5 |

Contributor: Joakim Ögren, Anselm Belz

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08