# Cisco Console (9)

Use this cable to configure a Cisco device using the Console port.

(To Computer).
(to the Cisco device)

9 PIN D-SUB FEMALE to the Computer
RJ45 MALE CONNECTOR to the Cisco device.

| DB9F | RJ45 | Dir
--- | --- | --- | ---
Receive Data | 2 | 3 |
Transmit Data | 3 | 6 |
Data Terminal Ready | 4 | 7 |
Ground | 5 | 4 |
Ground | 5 | 5 |
Data Set Ready | 6 | 2 |
Request to Send | 7 | 8 |
Clear to Send | 8 | 1 |

Contributor: Joakim Ögren, Damien Miller Dave Peverley

Source:
Cisco Catalyst 1900 Series Installation and Configuration Guide v9.x

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-28