# C64 Power Supply

Available at the Commodore 64.

(at the computer)

7 PIN DIN 'O' FEMALE at the computer.

Pin | Name
--- | ---
1 | Shield Ground
2 | Shield Ground
3 | Shield Ground
4 | Not connected
5 | +5v In
6 | 9Vac in
7 | 9Vac in

Contributor: Rob Gill

Source:
Commodore 64 Programmers Reference Guide

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07