# MIDI Out

MIDI=Musical Instrument Digital Interface.

(at the peripheral)
(at the cable)

5 PIN DIN 180° (DIN41524) FEMALE at the peripheral.
5 PIN DIN 180° (DIN41524) MALE at the cable.

Pin | Name | Description
--- | --- | ---
1 | n/c | Not connected
2 | GND | Ground
3 | n/c | Not connected
4 | CSINK | Current Sink
5 | CSRC | Current Source

Contributor: Joakim Ögren

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07