# Serial Printer (25-25)

Use this cable between two a computer (DTE) and a printer (DTE) devices.

(To Computer).
(To Printer).

25 PIN D-SUB FEMALE to Computer.
25 PIN D-SUB FEMALE to Printer.

| D-Sub 1 | D-Sub 2 |
--- | --- | --- | ---
Receive Data | 2 | 3 | Transmit Data
Transmit Data | 3 | 2 | Receive Data
Clear To Send + Data Set Ready | 5 + 6 | 20 | Data Terminal Ready
Carrier Detect + Data Terminal Ready | 8 + 20 |  |
Ground | 7 | 7 | Ground

Contributor: Joakim Ögren

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08